# Setting Up Access Control for Fiber Channel

Without any Fiber Channel (FC) access control rules, all configured VTL devices are accessible over every available HBA port on the VTL host.

Access control rules can be used to restrict access to entire VTL instances, or specific drives/medium changer within a VTL instance to specific Host HBA ports. Access control rules can be used to even specify the incoming HBA port through which access is allowed.

×

Loading...