# Snapshot Configuration Properties of the Silk Storage Array

The Configuration tab contains snapshot configuration properties that affect the behavior of the storage array in your environment.

Property | Description
--- | ---
Snap Operation Retry Interval (in seconds) | The time interval (in seconds) after which the next mount operation is attempted. The default value is 60.
Snap Operation Retry Count | The number of retry attempts for a mount operation. The default value is 10.
Enable Diagnostic Logging | When selected, enables diagnostic logging. The default value is not selected.
Remote Snap MA | The client name of the MediaAgent that you want to designate as the Remote Snap MediaAgent. If you configure Remote Snap MediaAgent, then the array communications are routed through this MediaAgent.

×

Loading...