# Snapshot Configuration Properties of the HPE Nimble Storage / Nimble dHCI / HPE Alletra 6000 Series / HPE Alletra 5000 Series Storage Array

The Configuration tab contains snapshot configuration properties that affect the behavior of the storage array in your environment.

Property | Description
--- | ---
Snap Operation Retry Interval (in seconds) | The time interval (in seconds) after which the next mount operation is attempted. The default value is 60.
Snap Operation Retry Count | The number of retry attempts for a mount operation. The default value is 10.
Enable Diagnostic Logging | When selected, enables diagnostic logging. The default value is not selected.
CHAP Account | If using the CHAP authentication protocol for iSCSI login, select the CHAP Account credentials.

×

Loading...