# Deployment of Commvault Grid

Commvault Grid deployment involves the following steps:

1. Configure a static IP address for the Intelligent Platform Management Interface (IPMI) port
2. If your deployment model is Reference Architecture, then set up the required hardware.
3. If you have an existing Commvault environment, you can connect to the existing CommServe server.
4. Perform network configuration to deploy Commvault Grid nodes.

×

Loading...