# Configuring Network Throttle

In the Command Center, you can configure the data upload speed for backups and data download speed for restores. These values are defined by the Throttle send (upload) and Throttle receive (download) values on the laptop plan settings page. By default, the throttle send value is 5000 Kbps and the throttle receive value has no limit.

## Procedure

1. From the Command Center navigation pane, go to Protect > Laptops.

   The Laptops page appears.

2. To view laptop plans click the Plans tab.

3. In the Plan name column, click the laptop plan for which you want to configure the network throttle.

   The laptop page appears.

4. On the Overview tab, in the Network throttle section, click edit .

   The Network throttle dialog box appears.

5. Modify the default Throttle send and Throttle receive values.

   Tip

   To set a value for Throttle receive, remove the selection for the No limit check box.

6. Click SAVE.

×

Loading...