# System Requirements for the NetApp Storage Array

Before you configure your storage array, verify that your system meets the following requirements.

## Licenses

Install the following licenses.

Array | Snapshot Type | License
--- | --- | ---
NetApp | Snapshot | FlexClone, installation on the storage array SnapRestore, installation on the storage array
NetApp Open Replication | Replica | FlexClone, installation on the storage array SnapRestore, installation on the storage array SnapVault or SnapMirror for replication, installation on the primary storage array and on the secondary storage array For SnapMirrorCloud Replication: SnapMirror Cloud and S3 SnapMirror licenses For SnapLock Enterprise and Tamperproof: SnapLock Enterprise license

## Version and Firmware

Use the following version and firmware.

Array | Version and Firmware for 7-Mode | Version and Firmware for C-Mode
--- | --- | ---
NetApp | Product ONTAP / Data ONTAP ONTAP versions ONTAP 7.3.5 or later 7.3.x subversion ONTAP 8.2, 8.1, including subversions | Products ONTAP / Data ONTAP Cloud Volumes ONTAP ONTAP Select ONTAP ASA r2 ONTAP versions ONTAP 8.3 and 8.2P3 (or later patch level) including subversions Cluster-Mode ONTAP 8.2.1 NFS configurations require 8.2.1P1 or later patch level with fix for NetApp BURT 806823 ONTAP 9.18.1, 9.17.1, 9.16.1, 9.15.1, 9.14.1, 9.13.1, 9.12.1, 9.11.1, 9.10.1, 9.9.1, 9.8, 9.7, 9.6, 9.5, 9.4, 9.3, 9.2, 9.1, 9.0
NetApp Open Replication | N/A | Products ONTAP / Data ONTAP Cloud Volumes ONTAP ONTAP Select ONTAP versions ONTAP 9.18.1, 9.17.1, 9.16.1, 9.15.1, 9.14.1, 9.13.1, 9.12.1, 9.11.1, 9.10.1, 9.9.1, 9.8, 9.7, 9.6, 9.5, 9.4, 9.3, 9.2, 9.1, 9.0, 8.3.2

## Protocols

Use one of the following protocols.

Array | Protocol
--- | ---
NetApp | Fibre Channel iSCSI CIFS, NFS FCoE* NDMP
NetApp ONTAP ASA r2 | Fibre Channel iSCSI

*This protocol is field certified.

## Software

Install the following software.

Array | Required Software
--- | ---
NetApp | None
NetApp Open Replication | None

## Ports

- For snapshot-based operations, open port 443 (HTTPS) for communication between the NetApp server and CommServe computer, MediaAgent, access node or remote snapshot MediaAgent in your CommCell environment.

- For SnapDiff V2 and V3, open port 2049 (NFS) for communication between the NetApp server and CommServe computer, MediaAgent, access node, or remote snapshot MediaAgent in your CommCell environment to transfer the file list information over NFS.

- For NetApp open replication with SnapMirror cloud, open the following ports for communication between the NetApp cluster and the object store destination:

  - Port 443 (HTTPS) for all the vendors

  - Port 10443 (HTTPS) for StorageGRID.

  For StorageGRID port requirements, see Snap Configuration.

## Licenses for Commvault IntelliSnap for NetApp

When you install the CIFN Enabler License, the backup copy job that is run from the NetApp snap engine is excluded from the backup capacity license calculation.

×

Loading...