# System Requirements for the Hitachi Vantara Storage Array

Before you configure the storage array, verify that your environment meets the system requirements.

## Licenses

Install the following licenses.

Array | Snapshot Type | License
--- | --- | ---
Hitachi Vantara VSP using CCI Engine | ShadowImage | ShadowImage
Thin Image | Thin Image
Hitachi Vantara VSP using Targetless Snap (CCI) Engine | Thin Image | Thin Image

## Version and Firmware

Use the following version and firmware.

Array | Version and Firmware
--- | ---
Hitachi Vantara VSP using CCI Engine | VSP 5600H, 5600, 5500H, 5500, 5200H, 5200, 5100H, 5100 VSP E Series VSP F900, F700, F370, F350 VSP G900, G700, G370, G350 VSP G1500*, G1000, G800, G400, G200 VSP One Block 20 VSP One Block 85
Hitachi Vantara VSP using Targetless Snap (CCI) Engine | Hitachi Vantara version 80-02-23 or later

*Supported through Field Certification. Contact your Software Provider or Professional Services to see if the specific FCoE can be supported.

### Support for HTI and HTIA Snapshots

Array | VSP 5000 | VSP E Series | VSP F/G Series | VSP One Block 20 | VSP One Block 85
--- | --- | --- | --- | --- | ---
HTI | Yes | Yes | Yes | No | No
HTIA | Yes | Yes | No | Yes | Yes

## Protocols

Use one of the following protocols.

Array | Protocol
--- | ---
Hitachi Vantara VSP using CCI Engine | Fibre Channel
Hitachi Vantara VSP using Targetless Snap (CCI) Engine | Fibre Channel
Hitachi Vantara VSP One Block 20 | Fibre Channel iSCSI (Starting Innovation Release 11.42.80)

## Software

Install the following software.

Array | Required Software
--- | ---
Hitachi Vantara VSP using CCI Engine | RAID Manager 01-29-03/05 or later installed on client and proxy For VSM, use RAID Manager 01-32-03/01 or later, installed on client and proxy.
Hitachi Vantara VSP using Targetless Snap (CCI) Engine | RAID Manager 01-33-xx/xx or later installed on client and proxy
Hitachi Vantara VSM or GAD | RAID Manager version 01-32-03/01 or later installed on the Remote Snap MediaAgent
Remote Snap MediaAgent | RAID Manager version 01-29-03/05 or later on the Remote Snap MediaAgent

## Ports

You do not need to open any specific port.

×

Loading...