# Snapshot Configuration of the Dell PowerStore Storage Array

The Configuration tab contains snapshot configuration properties that control the behavior of the storage array in your environment.

Property | Description
--- | ---
Array Host Aliases | The array host aliases like NFC/CIFS interfaces.
Enable Diagnostic Logging | When selected, enables diagnostics logging.
Snap Operation Retry Count | The number of retry attempts for a snapshot operation operation. The default value is 6.
Snap Operation Retry Interval (in seconds) | The time interval (in seconds) after which a snapshot operation will no longer be retried. The default value is 10.
Remote Snap MA | The client name of the MediaAgent that you want to designate as the Remote Snap MediaAgent. For more information, see Remote Snap MediaAgent.
Use this performance policy for snap clone/mount operation | The name of a performance policy that you want to use when performing mount operations and backup copy operations. For example, low, medium and high.
Resume paused replication session during aux/replica copy job | Specify to resume the paused replication session during auxiliary copy and replication copy operations.

×

Loading...