# System Requirements for Active Peer Persistence with HPE

Before you configure Active Peer Persistence verify that your environment meets the following requirements.

Note

HPE active peer persistence is configurable only for the HPE Alletra Storage MP Snap engine.

## Version and Firmware

Use the following versions and firmware.

Array | Version and Firmware
--- | ---
HPE Primera | 4.6.1
HPE Alletra 9000 Series | 9.6.1
HPE Alletra Storage MP B10000 | 10.4.0

## Protocols

Use one of the following protocols.

Array | Protocol
--- | ---
HPE Alletra Storage MP / Primera / HPE Alletra 9000 Series / HPE Alletra Storage MP B10000 | Fibre Channel iSCSI

×

Loading...