# System Requirements for the NetApp E-Series/LSI Storage Array with REST API Support

Before you configure your storage array, verify that your environment meets the following requirements.

## Licenses

Install the following licenses.

Snapshot Type | License
--- | ---
PiT (Point-in-Time) | Enable the default Premium features

## Versions and Firmware

Use the following version and firmware.

Array | Version and Firmware
--- | ---
NetApp E-Series/LSI | NetApp E-Series E5712

## Protocols

Use one of the following protocols.

Array | Protocol
--- | ---
NetApp E-Series/LSI | Fibre Channel iSCSI

## Ports

For snapshot operations, open port 8443 (HTTPS) between the server computers, Proxy MediaAgents, and client computers.

×

Loading...