# Enabling the Navisphere CLI

You can enable the Navisphere CLI command for mount and unmount operations.

If you are using VNX snapshots with firmware versions 05.33.009.5.218 (VNX2 series) and 5.32.000.5.249 (VNX1 series), use the nOptimizeVNXSnap additional setting so that Navisphere CLI command runs the mount and unmount operations.

## Procedure

- To the client computer, add the additional setting as shown in the following table.

  For instructions on adding additional settings from the CommCell Console, see Adding or Modifying Additional Settings from the CommCell Console.

Property | Value
--- | ---
Name | nOptimizeVNXSnap
Category | EventManager
Type | Integer
Values | 0: Not enabled 1: Enabled

×

Loading...