# Commvault Edge Reference Architecture Technical Specifications

Commvault validated reference design documents deliver tested configurations with leading hardware vendors to provide validated designs, complemented by best practices and configurations which will accelerate ROI, and reduce complexity.

Validated design specifications for the following servers are available:

Components | Specifications
--- | ---
Vendor | Dell HPE Lenovo
Hardware Models | Dell R660xs Dell R760 HPE DL320 Gen 11 HPE DL360 (Gen 10 or Gen 10+) HPE DL380 Gen 10, Gen 10 Plus, or Gen 11 Lenovo SR630V3
Minimum CPU cores | 16 or more cores, regardless of socket count (Intel Xeon 3rd gen Silver minimum)
Memory | 64GB RAM, minimum
Boot Device | 240GB or larger There must be a dedicated boot device with a Hardware RAID 1 configuration, preferably 2 x SSD/NVMe devices. Software RAID, such as VROC, are not supported.
Hardware RAID Controller | Dell H755 Dell H965i HPE Smart Array P816i HPE Smart Array P408i HPE Smart Array E208i HPE Broadcom MR216i HPE Broadcom MR416i Lenovo 5350-8i
NVMe/SSD Flash Device | 960GB minimum cache size for up to 50TB usable ROBO capacity 1.6TB minimum cache size for 50-75TB ROBO capacity 3.2TB minimum cache sizefor 75-150TB ROBO capacity
Storage Pool Data | Up to 12 drives may be configured in a supported Hardware Model Up to 20TB capacity per drive supported Configure hardware RAID volumes for the data drives
Network | Broadcom 57414 Dual Port 10/25Gb SFP+ or SFP28 card Broadcom 57504 Quad port 10/25Gb Broadcom 57416 Dual port 10Gb Base-T card Intel XL710 2-port 10G SFP+ Intel X710 Quad Port 10Gb SFP+ Intel XXV710 Dual Port 10/25Gb SFP28 Intel X520 Dual SFP+ 10 Gb NIC Mellanox MCX4121A-ACUT Dual port 10/25Gb SFP28 Mellanox MCX512A-ACAT ConnectX-5 EN Adapter Card 10/25GbE
Fiber HBAs | Qlogic 2772 Dual port 32Gb Fiber HBA Qlogic 2692 Dual port 16Gb Fiber HBA Emulex LPE35002 Dual port 32Gb Fiber HBA Emulex LPE31002 Dual port 16Gb Fiber HBA

×

Loading...