# Configuring the IBM FlashSystem Storage Array on the Array Software

Before using the IntelliSnap feature in the Commvault software, configure environment for the array.

## Procedure

1. On the proxy computers, map an exclusive and temporary logical unit number (LUN) to access the storage device.

2. Create a host for the client computer or for the proxy computer and then, do one of the following:

   - Add a host port (WWPN) for Fibre Channel.

   - Add the iSCSI host IQN.

3. If you are using firmware 8.3.X or later, do one of the following:

   - Turn the volume protection feature off.

   - Create a separate child pool for Commvault, turn the volume protection option off at the child pool level, and then, in the Commvault, specify the child pool in the snapshot configuration properties.

## Related Topics

- To read about disabling volume protection, go to the IBM Knowledge Center website and search for 'disabling volume protection'.

×

Loading...