# Snapshot Configuration of the Dell PowerFlex Array

The Configuration tab contains snapshot configuration properties that affect the behavior of the storage array in your environment.

Property | Description
--- | ---
Snap Operation Retry Interval (in seconds) | The time interval (in seconds) after which a snapshot operation will no longer be retried. The default value is 60.
Snap Operation Retry Count | The number of retry attempts for a snapshot operation operation. The default value is 30.
Enable Diagnostic Logging | When selected, enables diagnostics logging.
Host IP Group | The data IP address and the management IP address that are available on the ESX server.

×

Loading...