# Getting Started with the NetApp E-Series/LSI Storage Array

To set up the NetApp E-Series/LSI storage array, review system requirements, and then add the array in the Commvault software. Then you can modify the snapshot properties.

Note

Starting from Commvault Platform Release 2024E (11.36), the NetApp E-series/LSI Snapshot engine and NetApp E-series/LSI Volume Copy engines have been deprecated. The NetApp E-series PiT snap engine now uses REST APIs to perform snapshot operations. For more information, see NetApp E-Series/LSI PiT Snap Engine Migration from SMI-S Protocol to REST APIs.

## Procedure

1. Verify that your environment meets the following System Requirements.

   - Systems Requirements for NetApp E-Series/LSI Storage Array with REST API Support

   - Systems Requirements for NetApp E-Series/LSI Storage Array with SMI-S Protocol

2. On Commvault software, add and configure the NetApp E-Series/LSI storage array. See Setting Up the NetApp E-Series/LSI Array.

3. To customize the array to your environment, edit the Snap Configuration Properties of NetApp E-Series/LSI.

   NetApp E-Series/LSI storage array is now ready to operate.

4. Choose a Supported Agent to work in conjunction with the NetApp E-Series/LSI storage array.

×

Loading...