# Image and Register Air Gap HyperScale X Nodes

During imaging of each Air Gap HyperScale X node:

1. Configure only the following networks:

   - CommServe Registration
   - Storage Pool

2. Complete HyperScale X installation. For intrsuctions, see Getting Started With HyperScale X.

3. Register each node with the CommServe.

Note

Do not configure replication or additional data networks at this stage.

×

Loading...