# Commvault Flex Appliance Server Hardware Requirements

Component | 1U | 2U
--- | --- | ---
CPU | 32 Cores (2× Intel Xeon Silver) | 32 Cores (2× Intel Xeon Silver)
Memory | 256 GB | 256 GB
Boot storage | 2× 480 GB SSD/NVMe | 2× 480 GB SSD/NVMe
Cache (Index and DDB) | 15.36 TB NVMe | 15.36 TB NVMe
On-board network connectivity (Dell) | 4 × 100 GbE Ethernet QSFP56 | 4 × 100 GbE Ethernet QSFP56
On-board network connectivity (HPE) | 4 × 100 GbE Ethernet QSFP28 | 4 × 100 GbE Ethernet QSFP28
Network transceivers | Available at purchase | Available at purchase
Power supply (Dell, LOT 9 compliant) | 1100 W Titanium | 1100 W Titanium
Power supply (HPE, LOT 9 compliant) | 800 W Titanium | 800 W Titanium
Warranty coverage | Same or next business day, selected at time of purchase | Same or next business day, selected at time of purchase
Commvault Flex node (Dell) | Dell PowerEdge R660 | Dell PowerEdge R760
Commvault Flex node (HPE) | HPE DL360 Gen11 | HPE DL380 Gen11

Note

- Each node is designed to support up to 500 TB of backend storage. A minimum of two nodes is required to create the initial pool, ensuring redundancy.
- The solution includes four 100 Gbps NIC ports. These ports can also be used at 25 Gbps by using a breakout cable (not included).
- The primary difference between the 1U and 2U server configurations is the number of available PCIe slots. The default configuration uses the 1U server. If additional expansion cards are required, a 2U server may be needed. This is determined at the time of ordering.

×

Loading...