# Getting Started with the Fujitsu ETERNUS AF / DX Storage Array

To set up the Fujitsu ETERNUS AF / DX Storage Array, review system requirements, and then add the array in the Commvault software. Then you can modify the snapshot properties.

## Procedure

1. Verify that your environment meets the Systems Requirements.

2. Run scripts and configure the array in the array console before configuring the array in the Commvault software:

   - Review best practices

   - Configuring Fujitsu ETERNUS AF / DX on the Array Console

3. On Commvault software, add and configure the Fujitsu ETERNUS AF / DX storage array in IntelliSnap Arrays page. See Setting Up the Fujitsu ETERNUS AF / DX Array Using Arrays Page.

4. To customize the array to your environment, edit the Snap Configuration Properties of Fujitsu ETERNUS AF / DX.

   Fujitsu ETERNUS AF / DX storage array is now ready to operate.

## Where to Go from Here

Configure the destination volumes before any snap operation and choose one of the following agents to work in conjunction with the Fujitsu ETERNUS AF / DX storage array.

- Configuration of Destination Volumes

- Supported Agents

×

Loading...