# Configuring the Fujitsu ETERNUS AF / DX Storage Array on the Array Software

On the array software, verify that you have the following configuration.

## Procedure

- Enable the SMI-S (Storage Management Initiative Specification).

- Create a Host Affinity group for the client computer and proxy computers.

- Clear the IPv6 network settings in the Fujitsu ETERNUS AF / DX software. Snapshots or clones cannot be created when the IPv4 protocol is used and the IPv6 network settings are not cleared.

×

Loading...