# Configuring Continuous Replication for VMs Using HPE Zerto

To protect your VM data during a potential disaster or planned downtime, Commvault provides a lightweight integration with HPE Zerto. This integration allows you to launch the Zerto portal directly from the Command Center to configure and monitor continuous replication workflows.

## Deploy Zerto Virtual Manager Appliance

Deploy the Zerto Virtual Manager (ZVM) appliance and get the URL to the management interface. For more information, see ZVM Appliance Requirements, Supported Features & Configurations.

## Configure Access to Zerto in Commvault

To enable Zerto portal access from the Command Center, configure the following CommCell setting:

1. From the Command Center navigation pane, go to Manage > Settings > Advanced.

2. Click the Additional settings tile.

3. Click Add, and then select CommCell settings.

4. In the Name box, enter zertoConsoleUrl, and then select the name from the suggestion list.

   Note

   The name of the setting must be specified as zertoConsoleUrl. This value is case-sensitive.

5. In the Category box, select CommServDB.GxGlobalParam.

6. In the Type box, select String.

7. In the Value box, enter the ZVM appliance management interface URL.

8. Select the Enable checkbox, and then click Save.

## Launch Zerto Interface

To access the Zerto portal, click the HPE logo in the top-right corner of the Command Center screen. This will open the Zerto management interface portal where you can configure continuous replication for your VMs.

×

Loading...