# Configuring the Dell EMC VNX / CLARiiON Storage Array on the Array Software

To configure an Dell EMC VNX / CLARiiON storage array on the array software, enable Access Logix, configure the necessary storage, create the CLARiiON host database file, and then authorize the CLARiiON connection.

## Procedure

1. For the CX series, enable Access Logix.

   For VNX arrays, Access Logix is enabled by default.

   For information about how to enable Access Logix, go to the Dell EMC communities website, and search for the following terms, without quotation marks: Logix enable.

2. Configure the storage needed for Dell EMC VNX / CLARiiON, see Configuring the storage needed for Dell EMC VNX / CLARiiON.

3. Create a CLARiiON host database file, see Creating the CLARiiON host database file.

4. Authorize CLARiiON connection, see Authorizing the CLARiiON connectivity.

×

Loading...