# Advanced Configuration for the Hitachi Vantara Storage Array

Verify if the client setup is correct for the Hitachi Vantara CCI Engine.

## Before You Begin

Ensure that you set the user privileges and the command device properties.

## Procedure

1. With the command device to test raidcom commands, create a horcm instance.

2. Start the horcm instance.

   If the instance fails to start, read the horcm logs.

3. After the horcm instance started successfully, type the following commands:

        raidcom -login –IM$[inst_no] -s $[serial]

       raidcom lock resource -resource_name meta_resource –IM$[inst no]
        -s $[serial]

       raidcom unlock resource -resource_name meta_resource –IM$[inst no]
        -s $[serial]

   where:

   - Inst_no is the horcm instance number.

   - Serial is the array’s serial number.

   If any of the above commands fails, read the horcm logs.

4. For Windows systems, type the following command:

       raidscan –x findcmddev 1-100

   If the command device is within the range, then the command returns a valid command device for the array.

×

Loading...