# Configuring System Files to Skip During an Archive Operation

You can use this additional setting that specifies the path to skip during an archive operation.

Note

This key needs to be used with extreme caution and is not recommended in regular scenarios. If any system specific files gets archived, it might leave the machine unusable.

## Procedure

1. To the client computer, add the sSTUB_PRUNE_EXCEPTIONS additional setting as shown in the following table.

   For instructions about adding an additional setting from the CommCell Console, see Adding an Additional Setting from the CommCell Console.

Property | Value
--- | ---
Name | sSTUB_PRUNE_EXCEPTIONS
Category | FileSystemAgent
Type | String
Value | /path/** For instance, by default, /var/ is skipped from archiving, and if /var/App/ and all its sub directories should be considered for archiving, then it should be configured as follows /var/App/**.

×

Loading...