# Remote Office Appliance RO1100 - Technical Specifications

SYSTEM CAPACITY (RAW) | 24 TB
SYSTEM CAPACITY (USEABLE) | 4.5 or 14.5 TB
M.2-BASED FLASH STORAGE | 150 GB
SATA SSD (DDB/INDEX CACHE) | 960GB
MEMORY | 96 GB DDR4
COMPUTE | 1 x Intel Xeon Silver 4110 8C 2.10 GHz
CHIPSET | Intel® C624
ON-BOARD NETWORK CONNECTIVITY | 6 x 1 GbE 1 x 1 GbE iRMC
OPERATING ENVIRONMENT | Microsoft Windows 2019 Server
OPTIONAL ADD-IN CARDS | 16 Gb Dual Port PCIe FC HBA 12Gb SAS Dual Port PCIe HBA 10GbE Dual Port PCIe NIC
WEIGHT | Up to 16 kg (up to 36 lbs) * It is recommended that the node be carried and racked by at least 2 people.
DIMENSIONS | 1 Rack Units 483 mm (Bezel) / 435 mm (Body) x 770.7 mm x 43 mm (19” (Bezel) / 17.1” (Body) x 30.3” x 1.7”)
MOUNTING RACK DEPTH | 748.2 mm 29.46”
POWER SUPPLY | 2 x hot-plug power supply for redundancy 450W hot-plug, 94% (Platinum efficiency), 100-240V, 50 / 60Hz
ACTIVE POWER (MAX. CONFIGURATION) | 883 watts
RATED VOLTAGE RANGE | 100 V to 240 V (Platinum) 200 V to 240 V (Titanium)
FREQUENCY | 50 Hz - 60 Hz
RECOMMENDED OPERATING TEMPERATURES | 5 - 35 °C (41 - 95 °F)

×

Loading...