# Technical Specifications for Commvault Grid Appliance Models

The following table lists the technical specifications for Commvault Grid Appliance models:

Component | N4 | N12 | N24
--- | --- | --- | ---
CPU | 16 Cores (2x Intel Xeon Silver) | 32 Cores (2x Intel Xeon Silver) | 32 Cores (2x Intel Xeon Silver)
Memory | 256 GB | 512 GB | 768 GB
Storage |  |  |
Supported Drive Size | 8 or 20 TB | 8 or 20 TB | 20 TB
Node Capacity (usable) | 17 or 41 (TiB)2 | 50 or 124 (TiB)2 | 248 (TiB)2
Boot | 2x 480GB SSD
Cache (CVFS) * | 3.2 TB Flash/NVMe/SSD (includes Logs space) | 3.2 TB Flash/NVMe/SSD | 3.2 TB Flash/NVMe/SSD
Logs (Index cache/DDB) * | 3.2 TB Flash/NVMe/SSD | 6.4 TB Flash/NVMe/SSD
Network |  |  |
On-board network connectivity | 4x 10/25GbE Ethernet SFP+ (default) or Base-T (optional)
| Network Transceivers | Dell - Default - 10/25GbE SFP28 85C SR Optic
HPE - Default 10 or 25Gbe SFP28 Optic (selected at time of purchase)
Add-in cards | Additional network or fiber channel available at time of purchase
Dual Power Supplies (LOT9 compliant) | Dell - 1100W Titanium | Dell - 1100W Titanium | Dell - 1100W Titanium
| HPE - 800W Titanium | HPE - 1800-2200W Titanium | HPE - 1600W Platinum
Warranty coverage | Same or next business day, selected at time of purchase
| Technical Guides |  |  |
Commvault Grid Appliances for Dell | Dell PowerEdge R660xs | PowerEdge R760 | PowerEdge R760xd2
Commvault Grid Appliances for HPE | HPE DL360 Gen 10 | HPE DL380 Gen 10 Plus | HPE Apollo 4200 Gen 10 Plus
| DL320 Gen 11 | DL380 Gen 11 |

## Related Links

Dell iDRAC User Guide

×

Loading...