# Basic Topology for HyperScale Edge

Basic topology provides the minimum required connections for the data protection network.

In this topology, the node requires connections to 1 - 10 GbE port for data protection network, which transfers data to and from the clients being protected and connect to the CommServe server.

Use this procedure to deploy the HyperScale Edge software using the HyperScale Edge ISO 3.2411 or higher version.

Note

Basic topology is the easiest option to setup and deploy. However, this setup does not provide network redundancy, and is recommended only for non-production use, or if you do not have the required port availability for redundant connections.

## Network Requirements

The following network names and IP addresses are required for the basic topology:

| Node
--- | ---
Data Protection Fully Qualified Domain Name* |
Data Protection IP Address* |
Data Protection Netmask* |
Data Protection Gateway* |
Data Protection DNS 1* |
Data Protection DNS 2 |
Data Protection DNS 3 |
Data Protection NIC Port 1 Card 1 MAC Address |
Data Protection NIC Port 1 Card 2 MAC Address |

## CommServe Requirements

You will require the following information to connect to an existing CommServe server:

CommServe hostname (FQDN) | Fully qualified hostname (FQDN) associated with the existing CommServe server. Note TCP Ports 8400 & 443 must be open from the nodes to the CommServe server.
Username | Username associated with the admin user.
Password | Password for the admin user.

×

Loading...