# Supported Hardware Storage Arrays and Cloud Platforms

In V11 SP15, the names of the array vendors and engines are updated in both the Commvault software and the documentation. For more information, see Array Vendor Names and Engine Names.

Commvault Systems, Inc. tests major versions and some minor versions of firmware, so the best practice is to use the supported versions listed in this topic. If you encounter a problem with a minor version during an IntelliSnap operation, contact Commvault Systems, Inc..

IntelliSnap backup is designed to work in conjunction with the following storage arrays/cloud platforms that provide snapshot functionality for data protection operations:

Vendor | Snapshot | Version or Firmware | Licensing | Software | Protocol | Notes/Caveats
--- | --- | --- | --- | --- | --- | ---
Amazon Web Services | EBS Snapshot | None | None | None | None | Supported for Linux file system, Oracle agents, SAP HANA agents, SAP for Oracle agents, and Virtual Server Agent for Amazon.
Amazon FSx for NetApp ONTAP | Snapshot | ONTAP 9.18.1, 9.17.1, 9.16.1, 9.15.1, 9.14.1, 9.13.1, 9.12.1, 9.11.1 |  |  | CIFS, NFS iSCSI | If the volume of the file server that contains the LUN has a SnapMirror Synchronous (SM-S) relationship configured, then IntelliSnap operations on that LUN are not supported. NetApp Open Replication with SnapMirror Cloud is not supported. The storage array is a NetApp OEM partner and uses NetApp Snap engine.
Azure NetApp Files | Snapshot |  |  |  | CIFS NFS SAP HANA requires the NFSv4.1 protocol according to Microsoft and SAP requirements. |
Cisco HyperFlex | Snapshot | HXDP 5.0.2g HXDP 5.0.1b HXDP 4.5.2a HXDP 4.5.1a HXDP 4.0.2a HXDP 4.0.1b HXDP 3.5.2a HXDP 3.0.1e | None | In the guest VM, install the most recent VM tool | NFS 3 | Cisco HyperFlex array does not support IntelliSnap backups of independent disks, RDM disks, or shared disks. The reconciliation operation is not supported.
DataCore SANsymphony-V | Snapshot Clone | SANsymphony -V version 10.0 PSP3 and later SANsymphony-V version 9.0 PSP4 Update 4 and later |  | Microsoft .net framework 4.7 or later | Fibre Channel iSCSI | Supported on Windows(x64), Hyper-V, and VMware.
Dell EMC Isilon/PowerScale | Snapshot | OneFS 9.13 through 7.0 | SnapshotIQ License |  | CIFS, NFS NDMP | The support for the CIFS/NFS protocols is for network share backups only. The revert operation is not supported.
Dell PowerStore | Snapshot | PowerStore T 1.0.2, 1.0.4 PowerStore 2.1.1, 2.0.1, 2.0.0 PowerStore 4.2, 4.1, 4.0, 3.6, 3.5.0.1, 3.2.0.0, 3.0.0.1 | None | None | Fibre Channel iSCSI NFS | None
Dell PowerFlex | Snapshot | VR2_6.10000.123 R3_6.100.102 R3_5.1300.111 R2_0.11000.0 | None | ScaleIO Data Client (SDC) drivers on the client computer and proxy computer where snapshots are mounted. | ETH/IB | Supported on Windows(x64), Hyper-V, and VMware. Commvault software does not support hardware snap revert for the versions - R3_6.100.102 and R3_5.1300.111.
Dell EMC Storage Center (DSM) | Snapshot using DSM | 7.5.1, Dell EMC Storage Manager 2020 R1 build 20.1.1.716 7.4.2, Dell EMC Storage Manager 2019 R1 build 19.1.579 7.3.2.48 Dell EMC Storage Manager (DSM) 2018 R1.10 build 18.1.10.171 7.2.11.4, Dell EMC Storage Manager 2016 R3.20 build 16.3.20.22 | Data Instant Replay (snapshots) Remote Instant Replay (replication) Live Volume | Dell EMC Storage Manager: Dell EMC Storage Manager client, Dell EMC Storage Manager data collector, and Dell EMC Storage Manager Server | Fibre Channel iSCSI | Supported on Windows, Linux, VMware, and Hyper-V. The replication feature is not supported. Compellent Live Volume supported with DSM. The Microsoft Hyper-V agent is not supported with the metro cluster configuration.
Dell EMC Unity | Snapshot | Firmware: 5.5, 5.4, 5.3.1, 5.2.0, 5.1.2.0.5.007, 5.0.6.0.5.008, 5.0.3, 5.0.2.0.5.009, 4.5.1, 4.4.0, 4.3.1, 4.2.1, 4.1.2, 4.1.0 Models: Unity 600/500/400/300 Unity 650F/550F/450F/350F Unity VSA | Enterprise license |  | CIFS, NFS Fibre Channel LUN over iSCSI NDMP | Dell EMC Unity does not support the revert operations. Support for the CIFS protocol and the NFS protocol is for network share backups only. NDMP: Snapshot cataloging and live browse operations are supported only if the Linux/UNIX shares (NFS) option or the Multiprotocol Shares (SMB and NFS) option is selected while creating the File System in the Dell EMC Unity Filer. Browsing from a backup copy is supported for File Systems created using NFS, SMB, or multiprotocol.
Dell EMC VBLOCK/VxBLOCK |  | VxBLOCK 1000 | None | None |  | Refer to the specific storage array support section for Snapshot and Protocol information.
Dell EMC PowerMAX VMAX All Flash/ VMAX3 | Dell EMC TimeFinder SnapVX Dell EMC TimeFinder VP Snap Dell EMC TimeFinder Clone | PowerMAX VMAX All Flash VMAX3 | TimeFinder SnapVX TimeFinder VP Snap TimeFinder Clone Solutions Enabler Licensing | For the TimeFinder SnapVX(SYMCLI) engine, Solutions Enabler 10.0.0.5, 9.x on client and proxy computers or on Remote MA For the TimeFinder SnapVX engine, Solutions Enabler 9.x on SMI-S server For the TimeFinder VP Snap and TimeFinder Clone engines, Solutions Enabler 9.x on client and proxy computers or on Remote MA and Solution enabler 9.x on SMI-S server | Fibre Channel iSCSI for TimeFinder SnapVX only FCoE (Fibre Channel over Ethernet)* |
Dell EMC VMAX | Dell EMC TimeFinder VP Snap Dell EMC TimeFinder Clone Dell EMC TimeFinder Snap Dell EMC TimeFinder BCV | VMAX | TimeFinder VP Snap TimeFinder Clone TimeFinder Snap TimeFinder Mirror Solutions Enabler Licensing | For the TimeFinder SnapVX(SYMCLI), Solutions Enabler 10.0.0.5, 9.x on client and proxy computers or on Remote MA. For the TimeFinder SnapVX, Solutions Enabler 9.x or 8.x on the SMI-S server. For the TimeFinder VP Snap, TimeFinder Snap, TimeFinder Clone and TimeFinder BCV engines, Solutions Enabler 9.x, 8.x or 7.6.2.8 on client and proxy computers. | Fibre Channel FCoE (Fibre Channel over Ethernet)* | Remote SymApi Server is not supported. Client Components (SYMCLI) are required only during the initial one-time configuration. Base Components (with SYMAPI) are required for all snapshot operations. SYMCLI and SYMAPI do not need to be installed on source host when Remote Snap MA is configured for VMAX.
Dell EMC Symmetrix | Dell EMC TimeFinder Clone Dell EMC TimeFinder Snap Dell EMC TimeFinder BCV | DMX3 and later | Licenses for: TimeFinder Clone TimeFinder Snap TimeFinder Mirror Solutions Enabler Licensing | Solutions Enabler 6.4 or later on client and proxy computers | Fibre Channel FCoE (Fibre Channel over Ethernet)* | Remote SymApi Server is not supported. Client Components (SYMCLI) are required only during the initial one-time configuration. Base Components (with SYMAPI) are required for all snapshot operations. SYMCLI and SYMAPI do not need to be installed on source host when Remote Snap MA is configured for VMAX.
Dell EMC VNX | SnapView Snap SnapView Clone VNX Snapshots | VNX 7500, 5700, 5500, 5300, 5100 VNX 8000, 7600, 5800, 5600, 5400, 5200 VNX OE for Block Version 05.32 and later is required for VNX Snapshots | VNX Local Protection Suite | Solutions Enabler 7.6.2, on client and proxy computers Navisphere CLI on client and proxy computers (only required for VNX snapshots) Navisphere/Unisphere Host Agent on Client and Proxy | Fibre Channel iSCSI | VMware with NFS datastores are supported. Client Components (SYMCLI) are required only during the initial one-time configuration. Base Components (with SYMAPI) are required for all snapshot operations. For configuring a VNX array, refer to the step-by-step instructions provided for EMC CLARiiON. Hyper-V and UNIX are supported through Field Certification* for VNX 8000, 7600, 5800, 5600, 5400, 5200. Solutions Enabler 7.6.2 is the only supported version.
Dell EMC VNX / CLARiiON | SnapView Snap SnapView Clone | CX500 / CX700 CX4-120 - CX4-960 CX3-10 - CX3-80 | VNX Local Protection Suite | Solutions Enabler 7.6.2, on client and proxy computers Navisphere Host Agent on client and proxy computers | Fibre Channel FCoE (Fibre Channel over Ethernet)* | Client Components (SYMCLI) are required only during the initial one-time configuration. Base Components (with SYMAPI) are required for all snapshot operations. Solutions Enabler 7.6.2 is the only supported version.
Dell EMC VNX / Celerra | SnapSure Snap | DART 5.5 and later | SnapSure Snap License Solutions Enabler Licensing | Solutions Enabler 6.5.1 or later, except Solutions Enabler 8.x, on client and proxy computers Navisphere CLI on client and proxy computers | NFS NDMP CIFS |
Dell EMC VPLEX | Snapshot Clone | GeoSynchrony® 6.2, 6.1.0.1, 6.0 Metro node 9.0, 8.0, 7.1 |  | On the client or on the Remote Snap MA: Python 3.11.4, 3.9.11, 3.9.6, 3.9.2, 3.8.1, 3.6.4, 2.7, 2.6 On UNIX: openssl-devel package | Fibre Channel | Considerations for the EMC VPLEX Storage Array
Dell EMC XtremIO | Snapshot | XMS versions 6.3.3-8, 6.3.0-62, 6.0.2-17, 4.2.1 Build 8, 4.2.0 Cluster versions 4.0.2 Build 80, 4.0.15-24 For the XtremIO X2 Model: XMS version 6.3.3-8, 6.2.0-85 Build 85, 6.0.2-17, 6.0.1-30 Build 30 Cluster version 6.3.3-8_X2, 6.3.0-62_X2, 6.2.0-85_X2, 6.0.2-17, 6.0.1-27_X2 |  |  | Fibre Channel iSCSI |
Fujitsu ETERNUS AF / DX | SnapOPC Snap EC Clone SnapOPC+ Snap | ETERNUS AF S3 V11L20-0000, and later ETERNUS AF S3 series – 650, 250, 150 ETERNUS AF S2 V10L80-2000, and later ETERNUS AF S2 series – 650, 250 ETERNUS AF V10L60-0000, and later ETERNUS AF series – 650, 250 ETERNUS DX S6 V12L10-0000, and later ETERNUS DX S6 series – 8900, 900, 600 ETERNUS DX S5 V11L20-0000, and later ETERNUS DX S5 series – 900, 600, 500, 200, 100, 60 ETERNUS DX S4 V10L80-2000, and later ETERNUS DX S4 series – 600, 500, 200, 100, 60 ETERNUS DX S4 V11L20-0000, and later ETERNUS DX S4 series – 8900 ETERNUS DX S3 V10L60-0000, and later ETERNUS DX S3 series – 8900, 8700, 600, 500, 200F, 200, 100, 60 ETERNUS DX S2 series – 440, 410, 90, 80 | Local Copy Thin Provisioning | None | Fibre Channel iSCSI |
FUJITSU Storage ETERNUS AC/AX/HX Series | Snapshot | Cluster-Mode: ONTAP / Data ONTAP ONTAP 9.18.1, 9.17.1, 9.16.1, 9.15.1, 9.14.1, 9.13.1, 9.12.1, 9.11.1, 9.10.1, 9.9.1, 9.8, 9.7 Note The Active IQ Unified Manager (AIQUM) 9.14 and 9.13P1 are not supported. If you are using AIQUM-based replication, Commvault recommends verifying support from NetApp Interoperability Matrix for ONTAP 9.14.1, 9.15.1, 9.16.1, 9.17.1, and 9.18.1 with AIQUM 9.13* or older. For information on why certain AIQUM versions are not supported, see the NetApp KB articles CAIQUM-5577 and CAIQUM-6267. | FlexClone SnapRestore SnapVault or SnapMirror for replication, installation on the primary storage array and on the secondary storage array For SnapMirrorCloud Replication: SnapMirror Cloud and S3 SnapMirror licenses | To create SnapVault and SnapMirror copies of clustered Data ONTAP snapshot copies, use AIQUM (formerly OCUM) 9.18, 9.16P2**, 9.13*, 9.12*, 9.11*, 9.10, 9.9, 9.8, 9.7. To verify the latest support for your product, see NetApp Interoperability Matrix Tool. For SnapVault and SnapMirror configurations, if you are using ONTAP 19.18.1, 9.16.1, 9.13.1, 9.12.1 or 9.11.1, you can use AIQUM 9.18, 9.16P2 **, 9.13*, 9.12* or 9.11* respectively. *The AIQUM version is supported only with specific NetApp patches. For information on the AIQUM version, see the NetApp article and contact NetApp. **The AIQUM version is field certified. for more information, see the NetApp KB article. | CIFS, NFS Fibre Channel FCoE (Fibre Channel over Ethernet)* iSCSI NDMP | Supported on HP-UX running on Intel Itanium processors using Fibre Channel. For ONTAP 9.7 and later, if the volume of the file server that contains the LUN has a SnapMirror Synchronous (SM-S) relationship configured, then IntelliSnap operations on that LUN are not supported. The storage array is a NetApp OEM partner and uses NetApp Snap engine.
Google Cloud | Snapshot | None | None | None | None |
Hitachi NAS | Snapshot | 15.5, 15.4, 15.3, 15.2, 15.1, 14.9, 14.8, 14.7, 14.6, 14.5, 14.4, 14.3, 14.2, 13.9, 13.8, 13.7, 13.6, 13.5, 13.4, 13.3, 13.2, 13.0, 12.7 REST API Version 7.0, 4.0 | CIFS, NFS | For Hitachi NAS versions 13.2.x and later, use the in-built metro server. For Hitachi NAS earlier versions than 13.2.x , install an external metro server version 4.0. | CIFS, NFS NDMP | The support for the CIFS/NFS protocols is for network share backups only.
Hitachi Vantara VSP using CCI Engine | ShadowImage (SI) Thin Image (TI) | VSP 5600H, 5600, 5500H, 5500, 5200H, 5200, 5100H, 5100 VSP E Series VSP F900, F700, F370, F350 VSP G900, G700, G370, G350 VSP G1500*, G1000, G800, G400, G200 VSP One Block 20 VSP One Block 85 For information on HTI and HTIA snapshot support, see system requirements. | Thin Image ShadowImage | RAID Manager (01-29-03/05 and later) installed on client and proxy. For VSM, use RAID Manager (01-32-03/01 and later) installed on client and proxy. | Fibre Channel iSCSI | iSCSI protocaol is supported only with the Hitachi Vantara VSP One Block 20 array. This support is available starting Innovation Release 11.42.80. SI and TI of replicated volumes, Dynamic Provisioned volumes (DP-VOL) and External volumes (ELUN) are also supported. Hitachi Vantara VSP using CCI supports multi-array configuration. On Hitachi Vantara VSP G Series, mixed pools Hitachi Dynamic Provisioning (HDP) can contain Thin Image snapshots.
Hitachi Vantara VSP using Targetless Snap (CCI) Engine | Thin Image (TI) | Hitachi Vantara version 80-02-23 or later | Licenses for Thin Image | RAID Manager 01-33-xx/xx or later installed on client and proxy | Fibre Channel | Supports Windows agent and VMware agent. No support for replication. No support for snapshot of clone.
HPE Alletra 5000 Series | Snap and Replicate | 6.1.x | Included | None | Fibre Channel iSCSI | The storage array uses the HPE Nimble Storage Storage engine. Review Considerations for the HPE Nimble Storage Storage Array
HPE Alletra 6000 Series | Snap and Replicate | 6.1.x, 6.0.x | Included | None | Fibre Channel iSCSI | The storage array uses the HPE Nimble Storage Storage engine. Review Considerations for the HPE Nimble Storage Storage Array
HPE Alletra 9000 Series | Snapshot and Clone | 9.6.1* 9.5.21 9.5.18 9.5.15 9.5.7** 9.3.3 *If you have upgraded to HPE Alletra 9000 Series 9.6.1 version, ensure to set the SMIS Server Port to 5989 and enable Use secure connection to SMIS Server snapshot configurations. For more information, see snapshot configuration properties. | Virtual Copy | None | Fibre Channel iSCSI (firmware versions 9.5.15 and above) | The storage array uses the following engines: Snapshot: HPE Alletra Storage MP Snap Clone: HPE 3PAR StoreServ Clone HPE Alletra 9000 Series versions 9.5.4 and 9.5.3 are not supported.
HPE Alletra Storage MP B10000, powered by Alletra MP | Snapshot and Clone | 10.4.0** 10.3.0 10.2.0* *Supports only Linux and VMWare systems with iSCSI protocol. **Replication for this array version is not supported by Commvault due to the behavioral changes done by HPE in virtual volume sets and RCG. | Virtual Copy | None | Fibre Channel iSCSI | The storage array uses the following engines: Snapshot: HPE Alletra Storage MP Snap Clone: HPE 3PAR StoreServ Clone
HPE Primera | Snapshot and Clone | 4.6.1* 4.5.15.9 4.5.7.8** 4.4.1.7 4.3.3.2 4.2.1 4.0.1.3+1 (snapshot only) *If you have upgraded to HPE Primera 4.6.1 version, ensure to set the SMIS Server Port to 5989 and enable Use secure connection to SMIS Server snapshot configurations. For more information, see snapshot configuration properties. | Virtual Copy | None | Fibre Channel iSCSI | The storage array uses the HPE Alletra Storage MP Snap engine. HPE Primera versions 4.5.4 and 4.5.3 are not supported.
HPE Alletra Storage MP | Snapshot: HPE Alletra Storage MP Snap Clone: HPE 3PAR StoreServ Clone | 3.3.2.159(MU1) 3.3.1.648 (MU5) 3.3.1.410 (MU2)+P30, P32, 3.3.1.269 (MU1)+P08, P14, P17 3.2.2.709(MU6), 3.2.2.390 (EMU2), 3.2.2 (MU4), 3.2.2, 3.2.1 (MU3), 3.2.1 (MU2) 3.1.2 (MU3) 2.3.1 (MU4) | Virtual Copy Thin Provisioning (4096G) license is required when Thin Provisioning is enabled for cloning | None | Fibre Channel iSCSI | Considerations for the HPE Alletra Storage MP / Primera Storage Array
HPE XP 12000 (Hitachi Vantara OEM) | Business Copy | XP 24000 – 12000 | Business Copy | HPE StorageWorks Command View Advanced Edition Agent (Device Manager 7.1.1 or later), installed on client and proxy computers HPE StorageWorks Command View Advanced Edition Server (Device Manager 7.1.1 or later,) installed on any computer HPE StorageWorks RAID Manager, installed on client and proxy computers | Fibre Channel FCoE (Fibre Channel over Ethernet)* | The Virtual Machine HotAdd feature is not supported.
HPE XP P9500 (Hitachi Vantara OEM) | Fast Snap Business Copy | HPE XP P9500 70-06-58-00/00 | Fast Snap Business Copy | HPE RAID Manager 01.41.05 or later | Fibre Channel FCoE (Fibre Channel over Ethernet)* |
HPE XP7/XP8 (Hitachi Vantara OEM) | Fast Snap Business Copy | HPE XP8: 90-09-31-00/00 90-09-28-00/00 90-09-25-00/00 90-09-21-00/00 90-04-02-00/00 HPE XP7: 80-06-85-00/00 80-06-65-00/00 | Fast Snap Business Copy | HPE RAID Manager 01.41.05 or later | Fibre Channel FCoE (Fibre Channel over Ethernet)* |
HPE Nimble Storage | Snap and Replicate | 6.1.x, 6.0.x, 5.2.x, 5.1.x, 5.0.x, 4.x, 3.x Nimble CS-Series, AF-Series, and HF-Series | Included | None | Fibre Channel iSCSI | Considerations for the HPE Nimble Storage Storage Array
HPE Nimble dHCI | Snap and Replicate | 5.2.x Nimble AF-Series, and HF-Series | Included | None | iSCSI | Considerations for the HPE Nimble Storage Storage Array
Huawei OceanStor Convergent series | Snapshot Clone | Huawei OceanStor V3 Convergent Storage - V300R006C50, V300R006C30, V300R006C20, V300R006C10 Huawei OceanStor V5 Convergent Storage - V500R007 Huawei OceanStor Hybrid Flash Storage 6.1 | HyperSnap HyperClone Smart Thin (optional for Thin Clone) | None | Fibre Channel iSCSI CIFS, NFS | Considerations for the Huawei Storage Array Starting SP30, Commvault does not support firmware version V300R006C00. Commvault recommends you to upgrade to the latest firmware in case you have any issues.
Huawei OceanStor Dorado Series | Snapshot | Huawei OceanStor Dorado V6 – 6.1 Huawei OceanStor Dorado V3 - V300R001C00 Note Huawei OceanStor Dorado V6 HyperMetro Cluster only supports Microsoft SQL Server, Oracle, SAP HANA, VMware, Windows File System, and Unix File System agents. | HyperSnap | None | Fibre Channel iSCSI V6 only: CIFS, NFS | Considerations for the Huawei Storage Array
IBM N-Series | Snapshot | For 7-Mode: ONTAP 7.3.5 and later 7.3.x subversion ONTAP 8.2, 8.1, 8.0 including subversions For Cluster-Mode: ONTAP 8.3, 8.2P3 (and later patch level) including subversions Cluster-Mode ONTAP 8.2.1 NFS configurations require 8.2.1P1 and later patch level with fix for NetApp BURT 806823 ONTAP 9.18.1, 9.17.1, 9.16.1, 9.15.1, 9.14.1, 9.13.1, 9.12.1, 9.11.1, 9.10.1, 9.9.1, 9.8, 9.7, 9.6, 9.5, 9.4, 9.3, 9.2, 9.1, 9.0 Note The Active IQ Unified Manager (AIQUM) 9.14 and 9.13P1 are not supported. If you are using AIQUM-based replication, Commvault recommends verifying support from NetApp Interoperability Matrix for ONTAP 9.14.1, 9.15.1, 9.16.1, 9.17.1, and 9.18.1 with AIQUM 9.13* or older. For information on why certain AIQUM versions are not supported, see the NetApp KB articles CAIQUM-5577 and CAIQUM-6267. | FlexClone SnapRestore SnapVault or SnapMirror for replication, installation on the primary storage array and on the secondary storage array Operations Manager, Provisioning Manager, and Protection Manager licenses are required for OnCommand Unified Manager For SnapMirrorCloud Replication: SnapMirror Cloud and S3 SnapMirror licenses | To create SnapVault and SnapMirror copies of 7-Mode snapshots, use OnCommand Unified Manager server running OCUM 5.2, 5.1, or 5.0. For ONTAP 8.1, use OCUM 5.2 or 5.1. To create SnapVault and SnapMirror copies of clustered Data ONTAP snapshot copies, use OCUM 9.8, 9.7, 9.6, 9.5, 9.4, 7.3, 7.2, 7.1, 7.0, 6.4P1, 6.3P1, 6.2, 6.1, and 6.0, or AIQUM 9.18, 9.16P2**, 9.13*, 9.12*, 9.11*, 9.10, 9.9, 9.8, 9.7, and 9.6. To verify the latest support for your product, see NetApp Interoperability Matrix Tool. For SnapVault and SnapMirror configurations, if you are using ONTAP 19.18.1, 9.16.1, 9.13.1, 9.12.1 or 9.11.1, you can use AIQUM 9.18, 9.16P2 **, 9.13*, 9.12* or 9.11* respectively. *The AIQUM version is supported only with specific NetApp patches. For information on the AIQUM version, see the NetApp article and contact NetApp. **The AIQUM version is field certified. for more information, see the NetApp KB article. | CIFS, NFS Fibre Channel FCoE (Fibre Channel over Ethernet)* iSCSI NDMP | Supported on HP-UX running on Intel Itanium processors using Fibre Channel. The storage array is a NetApp OEM partner and uses NetApp Snap engine.
IBM FlashSystem | FlashCopy Space-efficient Flash Copy IBM Volume Group Snap | Supported models: V9000, V7000, V5200, V5100 Supported versions: 9.1.0.1, 8.7.0.0, 8.6.2.1, 8.6.0.2, 8.5.0.11, 8.5.0.7, 8.5.0.5, 8.4.0.2, 8.3.1.1, 8.2.1.8, 8.1.1.0, 7.8.1.3, 7.8.0.2, 7.8.1.1*, 7.7.0.2, 7.6.1.4, 7.6.0.3, 7.5.0.2, 7.4.1.2, 7.4.0.7*, 7.4.0.6*, 7.4.0.4*, 7.4.0.2, 7.3.0.11*, 7.3.0.9, 7.3.0.4 till 6.1.0.7 Note Starting IBM FlashSystem firmware version 8.6.2.x onwards, IBM has deprecated the use of SMI-S. Hence, if you have upgraded your firmware version to 8.6.2.1 or above, IntelliSnap operations will run using the REST API by default. The lower firmware versions will still use the SMI-S and opening REST API Port 7443 from Client/Proxy to the array is necessary as a prerequisite. | FlashCopy | None | Fibre Channel iSCSI | For the SAP HANA agent, there is support for the IBM Power PC (Little Endian) platform.
IBM XIV | Snap | XIV, A9000, and A9000R | Included | IBM XCLI 4.3 on client and proxy computers For models A9000 and A9000R, the IBM XCLI 5.1 and 5.0 versions are supported. | Fibre Channel iSCSI | For the SAP HANA agent, there is support for the IBM Power PC (Little Endian) platform. Supported on Windows 2012 R2 cluster.
INFINIDAT | Snapshot | Version 8.1.x, 7.3.x, 7.1.x, 7.0.x, 6.0.x, 5.5.x, 5.0.x, 4.0.x | Included | None | Fibre Channel iSCSI NFS (firmware versions 5.x and 4.x are not supported) |
Lenovo DE Series | PiT (Point-in-time) | 08.62.00.02 | Snapshot | SMI-S 11.62 | Fibre Channel iSCSI | PiT snap creation is not supported for the volumes involved in replication.
Lenovo DG Series | Snapshot | Cluster-Mode: ONTAP 9.15.1P2 ONTAP 9.16.1, 9.17.1, 9.18.1 | FlexClone SnapRestore SnapVault or SnapMirror for replication, installation on the primary storage array and on the secondary storage array For SnapMirrorCloud Replication: SnapMirror Cloud and S3 SnapMirror licenses | To create SnapVault and SnapMirror copies of clustered Data ONTAP snapshot copies, use AIQUM (formerly OCUM) 9.16P2* and 9.18. To verify the latest support for your product, see NetApp Interoperability Matrix Tool. *The AIQUM version is field certified. for more information, see the NetApp KB article. | CIFS, NFS iSCSI NDMP | If the volume of the file server that contains the LUN has a SnapMirror Synchronous (SM-S) relationship configured, then snapshot operations on that LUN are not supported. The storage array is a NetApp OEM partner and uses NetApp Snap engine.
Lenovo DM Series | Snapshot | Cluster-Mode: ONTAP / Data ONTAP ONTAP 9.18.1, 9.17.1, 9.16.1, 9.15.1, 9.14.1, 9.13.1, 9.12.1, 9.11.1, 9.10.1, 9.9.1, 9.8, 9.7 Note The Active IQ Unified Manager (AIQUM) 9.14 and 9.13P1 are not supported. If you are using AIQUM-based replication, Commvault recommends verifying support from NetApp Interoperability Matrix for ONTAP 9.14.1, 9.15.1, 9.16.1, 9.17.1, and 9.18.1 with AIQUM 9.13* or older. For information on why certain AIQUM versions are not supported, see the NetApp KB articles CAIQUM-5577 and CAIQUM-6267. | FlexClone SnapRestore SnapVault or SnapMirror for replication, installation on the primary storage array and on the secondary storage array For SnapMirrorCloud Replication: SnapMirror Cloud and S3 SnapMirror licenses | To create SnapVault and SnapMirror copies of clustered Data ONTAP snapshot copies, use AIQUM (formerly OCUM) 9.18, 9.16P2**, 9.13*, 9.12*, 9.11*, 9.10, 9.9. 9.8 or 9.7. To verify the latest support for your product, see NetApp Interoperability Matrix Tool. For SnapVault and SnapMirror configurations, if you are using ONTAP 19.18.1, 9.16.1, 9.13.1, 9.12.1 or 9.11.1, you can use AIQUM 9.18, 9.16P2 **, 9.13*, 9.12* or 9.11* respectively. *The AIQUM version is supported only with specific NetApp patches. For information on the AIQUM version, see the NetApp article and contact NetApp. **The AIQUM version is field certified. for more information, see the NetApp KB article. | CIFS, NFS Fibre Channel FCoE (Fibre Channel over Ethernet)* iSCSI NDMP | Supported on HP-UX running on Intel Itanium processors using Fibre Channel. For ONTAP 9.7 and later, if the volume of the file server that contains the LUN has a SnapMirror Synchronous (SM-S) relationship configured, then IntelliSnap operations on that LUN are not supported. The storage array is a NetApp OEM partner and uses NetApp Snap engine.
Microsoft Azure | Snapshot | None | None | None | None | Supported for the following agents: SAP Oracle, SAP HANA, and SQL Server.
NEC (Deprecated) | Snapshot (NEC DynamicSnapVolume) and Replication (NEC DynamicDataReplication) | NEC M-Series with Storage Control Software version 087C | None | NEC Storage Manager version 9.3.006 on the client computer | Fibre Channel |
NetApp | Snapshot | For 7-Mode: Product ONTAP / Data ONTAP ONTAP versions ONTAP 7.3.5 and later 7.3.x subversion ONTAP 8.2, 8.1, and 8.0 including subversions For Cluster-Mode: Product ONTAP / Data ONTAP Cloud Volumes ONTAP ONTAP Select ONTAP ASA r2 ONTAP versions ONTAP 8.3 and 8.2P3 (and later patch level) including subversions Cluster-Mode ONTAP 8.2.1 NFS configurations require 8.2.1P1 and later patch level with fix for NetApp BURT 806823 ONTAP 9.18.1, 9.17.1, 9.16.1, 9.15.1, 9.14.1, 9.13.1, 9.12.1, 9.11.1, 9.10.1, 9.9.1, 9.8, 9.7, 9.6, 9.5, 9.4, 9.3, 9.2, 9.1, and 9.0 ASA r2 requires ONTAP 9.17.1P2 Note The Active IQ Unified Manager (AIQUM) 9.14 and 9.13P1 are not supported. If you are using AIQUM-based replication, Commvault recommends verifying support from NetApp Interoperability Matrix for ONTAP 9.14.1, 9.15.1, 9.16.1, 9.17.1, and 9.18.1 with AIQUM 9.13* or older. For information on why certain AIQUM versions are not supported, see the NetApp KB articles CAIQUM-5577 and CAIQUM-6267. | FlexClone SnapRestore SnapVault or SnapMirror for replication, installation on the primary storage array and on the secondary storage array For OCUM 5.x: Operations Manager, Provisioning Manager, and Protection Manager licenses For SnapMirrorCloud Replication: SnapMirror Cloud and S3 SnapMirror licenses For SnapLock Enterprise and Tamperproof: SnapLock Enterprise license | To create SnapVault and SnapMirror copies of 7-Mode snapshots, use OnCommand Unified Manager server running OCUM 5.2, 5.1, or 5.0. For ONTAP 8.1, use OCUM 5.2 or 5.1. To create SnapVault and SnapMirror copies of clustered Data ONTAP snapshot copies, use OCUM 9.8, 9.7, 9.6, 9.5, 9.4, 7.3, 7.2, 7.1, 7.0, 6.4P1, 6.3P1, 6.2, 6.1, and 6.0, or AIQUM 9.18, 9.16P2**, 9.13*, 9.12*, 9.11*, 9.10, 9.9, 9.8, 9.7, and 9.6. To verify the latest support for your product, see NetApp Interoperability Matrix Tool. For SnapVault and SnapMirror configurations, if you use ONTAP 9.3, use OnCommand Unified Manager 7.3. If you are using ONTAP 9.13.1, 9.12.1 or 9.11.1, you can use AIQUM 9.13*, 9.12* or 9.11* respectively. *The AIQUM version is supported only with specific NetApp patches. For information on the AIQUM version, see the NetApp article and contact NetApp. **The AIQUM version is field certified. for more information, see the NetApp KB article. | CIFS, NFS Fibre Channel FCoE (Fibre Channel over Ethernet)* iSCSI NDMP | Considerations for the NetApp Storage Array
NetApp E-Series (LSI arrays) | PiT(Point-in-time) Snapshot (Deprecated) VolumeCopy (Deprecated) | Dell MD Series – 3220(i), 3200(i), 3000(i) IBM DS - 5300, 5100, 5020, 4800, 4700–4500, 4400, 4300, 4200, 4100, 3950, 3524, 3512–3400, 3300, 3200 NetApp E-Series E5712 NetApp E-Series E5500 SGI IS – 5xxx, 4xxx, 400, 350, 220 SGI TP – 9500(s), 9400(s), 9300(s) Sun - FLX280, FLX240, FLX210, 9176, 6780, 65xx, 61xx, 25xx | Snapshot VolumeCopy Legacy license for LSI Snapshot engine with NetApp E-series/LSI arrays | Rest API versions LSI SMI-S server versions 11.71, 11.52, 11.50, 11.42, 11.40, 10.34, 10.32.0G00.002, 10.30.0G00.009, 10.10.6054 | Fibre Channel iSCSI | VolumeCopy is not supported for Hyper-V. Snapshot and VolumeCopy do not support revert operations. Fibre Channel is not supported with SMI-S version 10.30. VolumeCopy is not supported for versions 11.52, 11.42, 11.40. PiT snap creation is not supported for the volumes involved in replication.
NetApp SolidFire | Snapshot | NetApp SolidFire Element OS 12.3, 12.2, 11.8, 11.7, 11.3, 11.1.0.72, 10.3, 10.0.0.282, 9.3, 8.0.1.2 NetApp HCI with Element OS 12.3, 12.2, 11.8, 11.7, 11.3, 11.1.0.72, 10.3 REST API Version 7.0 | None | None | Fibre Channel iSCSI | Supported on Linux, Microsoft Hyper-V, VMware, and Windows(x64) platforms. For the Linux platform, the iSCSI support is only on Red Hat Linux 7.x-5.5 and CentOS 7.x-5.5. For UNIX File System agent and database agents, NetApp SolidFire is supported only on the Linux OS.
Nutanix | Snapshot | Microsoft Hyper-V hypervisor: AOS 5.20, 5.19, 5.17, 5.15, 5.11, 5.10.x, 5.9.x, 5.5.x, 5.1.x, 5.0, 4.7, 4.6.x, 4.5.x Nutanix AHV hypervisor: AOS 6.0, 5.20, 5.19, 5.18x, 5.17.x, 5.15, 5.11, 5.10.x, 5.9.x, 5.6.x, 5.5.x, 5.1.x, 5.0, 4.7, 4.6.x, 4.5.x VMware hypervisor: AOS 7.0, 6.8, 6.5, 6.0, 5.20, 5.19, 5.18x, 5.17.x, 5.15, 5.11, 5.10, 5.8.x, 5.9.x, 5.5.x, 5.1.x, 5.0, 4.7, 4.6.x, 4.6, 4.5.x | None | None | NFS for VMware SMB3 for Hyper-V | IntelliSnap backup of single virtual machines hosted on multiple data stores is not supported. For streaming backups of VMs from a container that has the Nutanix Metro Availability feature enabled, use the NBD transport mode. If the MediaAgent used by the backup copy operation to mount snapshots goes down permanently, then those snapshots are left behind and there is no cleanup request sent from any other MediaAgent. For Nutanix VMWare: If performing container level hardware snapshots, use a Nutanix Snapshot as a Snap engine. If performing VM level hardware snapshots, use Nutanix VM Snap as an engine.
Oracle ZFS (Deprecated) | Snapshot | Snapshot ZS3-4, ZS3-2 with minimum firmware versions 7x20 (2011.1.4.2 for non-VMware & 2013.1.0.1 for VMware) | Separate cloning license per controller or node | None | Fibre Channel iSCSI | Supported on Windows (x64), Linux, Solaris, VMware, and Hyper-V.
Pure Storage FlashArray Files Snap | Snapshot | Product Pure Storage FlashArray Purity version 6.10.2 REST API version 2.49 | None | None | NFS | Limitations and considerations for Pure Storage FlashArray File (NFS)
Pure | Snapshot | Product Pure Storage FlashArray Cloud Block Store Purity version 6.10.2, 6.9.2, 6.8.9, 6.7.2, 6.5.2, 6.4.3, 6.3.6, 6.2.14, 6.1.10, 6.1.3, 5.3.10, 5.3.8, 5.3.6, 5.3.2, 5.2.3, 5.1.6, 5.1.1, 5.0.1, 4.10.9, 4.10.7, 4.9.6, 4.8.10, 4.8.7, 4.7.5, 4.6.11, 4.5.5, 4.1.1 REST API version 2.16, 1.4 | None | None | Fibre Channel iSCSI | For any of the Purity ActiveCluster releases from 5.0.5 to 5.0.0, when the source volume is externally deleted on the array and a snapshot of the source volume is mounted inside a pod, the source volume and the snapshot mount clone are deleted.
Silk Software Defined Cloud Storage (Azure) | Snapshot | 8.6.10 and later | None |  | iSCSI | Supported on the Windows, Linux, file systems and Microsoft SQL, Oracle databases. The Silk engine does not support the mapping of snapshots to an individual host VM that is part of a host group. Make sure that the VM that is used during snapshot mapping is not be part of any host group. The Silk Software Defined Cloud Storage (Azure) solution is cloud-platform agnostic. Azure is officially certified by Commvault. AWS and GCP are supported through Field Certification.
Tintri VMstore | Snapshot | 4.6.2.1-11182.55325.24595 4.3.2.4-9170.48932.21603 REST API version v310 | None | None | NFS 3.0 |
VAST Data Platform | Snapshot | 5.0.0.x | None | None | CIFS NFS |
Western Digital IntelliFlash | Snapshot | NFS for the VMware agent: INTELLIFLASH 3.11.0, 3.10.0, 3.9.1, 3.7 REST API 2.5, 2.4, 2.3, 2.1 NFS 4.0–2.0 For all other agents: INTELLIFLASH 3.11.0, 3.10.0, 3.9.1, 3.7, 3.5 REST API 2.5, 2.4, 2.3, 2.1, 2.0 | None | None | Fibre channel iSCSI NFS 2.0 -4.0 for the VMware agent |

*Supported through Field Certification. Contact your Software Provider or Professional Services to see if the specific FCoE can be supported.

**Replication for this version of array is pending validation by Commvault.

Notes

- Do not install the Commvault software on the same volume that you are protecting with the IntelliSnap backup feature.

- Subclients must contain LUNs (Logical Unit Number) from the same storage array. You can configure subclients with LUNs from multiple storage arrays of the same vendor for NetApp, Pure Storage FlashArray, and Hitachi Vantara VSP running the Hitachi Vantara CCI engine. Do not use this configuration on other storage vendors.

- NetApp storage arrays support LUNs from multiple NetApp storage arrays, if the subclients are on the same filer operating system. For example, LUNs from 7-Mode and LUNs from Cluster-Mode cannot be part of the same subclient.

- Commvault software supports IntelliSnap backups of subclients that have LUNs from multiple Hitachi Vantara VSP storage arrays that use Hitachi Vantara CCI engines.

- Migrated LUNs from IBM XIV are supported. For other storage arrays, contact the vendor for information.

- Most capabilities of Data ONTAP 7-Mode apply to Cluster-Mode, but cascaded replication of primary to snapvault to snapmirror on a single policy is not supported.

- Dynamic Disks on Window Operating Systems are not supported.

- When performing IntelliSnap backup for a Windows MSCS Cluster, a separate proxy server (external to the cluster nodes) must be used for mount, backup, and restore operations as disk signature conflicts might occur if these operations are performed from one of the servers in the cluster.

- Booting from SAN volumes is not supported.

- The IntelliSnap feature is not supported for VMware data stores created using local disks. The data stores should be created from LUNs.

- NAS attached tape libraries are not supported for IntelliSnap operations.

- The backup copy operation is not supported on a client computer that is upgraded to a version higher than its associated MediaAgent. For example, there is no support for backup copy operations if the client runs version 10 and the MediaAgent runs version 11.

- IntelliSnap backups of Raw Device Map (RDM) disks (passthrough disks for Hyper-V) are supported for all agents, but the Virtual Server Agent only provides support for VMware and Microsoft Hyper-V virtual machines:

  - For VMware, see Include RDMs and Independent Disks in IntelliSnap Backup Operations.

  - Hyper-V backups include passthrough disks if the following conditions are met:

    - The virtual machine has a File System agent or another supported agent installed on it and uses that agent for IntelliSnap backups.

    - The client computer (physical or virtual) is configured to mount snapshots using the iSCSI initiator, or the physical proxy server is configured to mount snapshots over Fibre Channel.

    - The passthrough disk on the virtual machine is attached using a virtual Fibre Channel adapter.

- For VMware VMs, the host of the virtual computer must have ESX server version 5.0 or later.

- Revert operation is not supported for LUNs configured as RDMs for the NetApp storage array.

- For NetApp arrays and arrays that use the NetApp Snap engine, if you are using AIX, HP-UX, or Solaris clients or access nodes, the following conditions apply:

  - For ONTAP versions earlier than 9.11.1, snapshot and other operations are not supported. However, you can configure and use a Windows or Linux-based remote MediaAgents or proxy access node to perform those operations.

  - For ONTAP versions 9.11.1 or later:

    - Snapshot and other operations are supported only if REST APIs are enabled on the array. For information on enabling REST APIs, see the How to enable REST API based authorization? section on Frequently Asked Questions for the NetApp Storage Array.

    - AIQUM based snapshot replication is not supported. However, you can configure and use a Windows or Linux-based data path MediaAgents for the storage policy copy to perform this operation.

×

Loading...