# Getting Started with NetApp Archiving

This topic describes the high-level steps that first-time users must follow to set up the archiving feature in the Command Center.

## Before You Begin

Configure Storage.

## Procedure

1. Verify that your access node meets the system requirements for NetApp archiving.

2. Verify that your share access nodes meet the following hardware requirements.

   A share access node is a computer that has access to the network shares and is used for live scan and archive operations.

   Component | Requirement
   --- | ---
   CPU/RAM10 | 2 CPU cores, 16 GB RAM (or 2 vCPUs/16 GB)
   OS or Software Disk | 200 GB usable disk, min 2 spindles 15KRPM

3. Install the Commvault software packages on your share access node.

4. Complete the filer archiving configuration for NetApp.

5. Create an archive plan.

6. Add the archiving file server to the Command Center.

   You can also configure an existing file server in the Command Center.

7. Create an archive set.

   Archive sets are logical groupings of subclients that contain data to be archived. You can create user-defined archive sets to manage specific data.

8. Optional: Create a subclient for archiving..

   Archiving subclients are logical containers of data to be archived. When you create an archive set, a default subclient is automatically created. The default subclient contains the data, plan, filters, and exceptions that you added when you created the archive set.

   You can create additional user-defined subclients to manage specific data.

9. Perform an archive operation.

   When you run an archive operation, the files that meet the archiving rules are stubbed.

10. Access your archived data.

×

Loading...