# Add Cartridges to the Virtual Tape Library

Add cartridges to the virtual tape library (VTL).

## Procedure

1. From the navigation pane, click Virtual Libraries.

   The Configured VTLs page appears.

2. In the View column for the VTL to which the cartridges must be added, click View.

   The VTL Information page appears.

3. Click Add VCartridge.

   The Add VCartridge dialog box appears.

4. From the Storage Pool list, choose the backup data storage pool to which the cartridges must be associated.

   Note

   This is not the default pool.

5. In the Number of Cartridges box, type the total number of cartridges that must be added.

   If necessary, configure additional options as described in Add Cartridges.

6. In the VCatridge Label/Prefix box, type a 6-digit label.

   - If the number of cartridges is greater than one, then the label will be of the following format:

     LTO000

     For example, if the number of cartridges is 2, then the labels for the newly created cartridges will be LTO000L6 and LTO001L6. If WORM is selected, then the labels for the newly created cartridges for our example will be LTO000LU and LTO0001LU.

   - If the number of cartridges is one, then the label can be a maximum of 32 characters.

   - Alphabets a-z, A-Z and numbers 0-9 are accepted as label/prefix.

     For example, if the number of cartridges is 4, then the labels for the newly created cartridges will be LTO000L6, LTO001L6, LTO002L6 and LTO003L6. If WORM is selected, then the labels for the newly created cartridges for our example will be LTO000LU, LTO0001LU, LTO002L6U, and LTO003L6U.

7. Click Submit.

   The newly added cartridges are displayed under VCartridge Information.

×

Loading...