# Configuring HPE Alletra Storage MP / Primera / HPE Alletra 9000 Series / HPE Alletra Storage MP B10000 Storage Array Using Arrays Page

For IntelliSnap backups from the Commvault software using either the HPE Alletra Storage MP, the HPE Primera, the HPE Alletra 9000 Series, or the HPE Alletra Storage MP B10000 storage array, add the HPE Alletra Storage MP storage array and its configuration information to the CommServe database.

## Before You Begin

For the Name box in the procedure below, you might need to calculate the storage array name, depending on the application that you are using to manage the storage array.

If you are using the StoreServ Management Console (SSMC) to manage your array or directly accessing array using service console, then you do not need to calculate the array name. In the Name box, enter the World Wide Name (WWN) of the storage system.

If you are using the old management console (InForm Management Console), then for the Name box, calculate the storage array name.

For the credentials below, the user type must be local user with edit and super level. The domain user is not supported.

## Start the Configuration Wizard

1. From the Command Center navigation pane, go to Manage > Infrastructure.

   The Infrastructure page appears.

2. Click Arrays.

3. On the Arrays page, click Add.

   The General page of the Add Snap Array configuration wizard appears.

## General

1. From the Snap vendor list, select HPE Alletra Storage MP.

2. In the Array name box, enter the WWN identifier of the storage array in upper case.

3. In the Control host box, enter the management IP address of the array.

4. In the Description box, enter the description for the array.

5. From the Saved credentials list, select the existing credentials or add new credentials you want to use.

   Steps to add new credentials

   To add credentials to the Credential Manager, click the plus button (+), and then specify the following in the Add Credential dialog box.

   1. In the Credential name box, enter the name of the credential.

   2. In the User account box, enter the name of the user account.

   3. In the Password box, enter the password.

   4. In the Description box, you can enter a description of the credentials.

   5. Click Save.

   Note

   Select or add the credentials of a user who has the Super User permission or the Edit User permission.

6. Click Next.

   The Array Access Nodes page of the configuration wizard appears.

## Array Access Nodes

Add an array access node if you want to use the secondary live snapshot for the backup copy operation or to add a MediaAgent to perform additional operations on the storage array.

1. From the Available MediaAgents list, select one or more access nodes and then click OK.

   - To select all the available MediaAgents as access nodes, click Select all.

2. To disable pruning, move the Pruning toggle button of the respective access node to the left.

3. To rearrange the selected access nodes, drag them upwards or downwards as required.

4. Click Next.

   The Snap Configurations page of the configuration wizard appears.

## Snap Configurations

1. Configure Snapshot Configuration Properties according to your needs.

2. Click Submit.

## Related Topics

- Configuring Array Access nodes

×

Loading...