# Setting up the Network for Linux CommServe Bare Metal

Setting up the network is the first phase in deploying the Linux CommServe Bare Metal node. All the network related information is required during this phase.

Note

Make sure to determine your network topology before setting up the network in your Linux CommServe Bare Metal node.

Network can be setup using one of the following configuration methods depending on the network topology for your environment:

Use one of the following configuration methods depending on the network topology for your environment:

- Basic Deployment

- Bonding (Active-Backup or LACP)

×

Loading...