# Naming Convention for Snapshots Created by the Fujitsu ETERNUS AF / DX Storage Array

The snapshots created by the Fujitsu ETERNUS AF / DX array have the following naming conventions.

Snapshot engine | Configuration | Naming convention | Example
--- | --- | --- | ---
Fujitsu ETERNUS AF / DX Clone | default | SP_2_JobID_SnapID | SP_2_5550_445
Fujitsu ETERNUS AF / DX Snap | default | SP_2_JobID_SnapID | SP_2_5559_4893
Fujitsu ETERNUS AF / DX SnapOPC+ | default | SP_2_JobID_SnapID | SP_2_5554_4874

where:

- SP_2 is a constant value.

- JobID is the Commvault software JobID.

- SnapID is the snapshot ID created by the Commvault software, and corresponds to the primary key of the SMSnap table entry in the CommCell database.

×

Loading...