# Configuring the Huawei HyperMetro Feature

To use the Huawei HyperMetro feature, you need to perform the configuration steps that HyperMetro Huawei documentation describes. On the Commvault software, you need to add the arrays in Array Management.

## Procedure

On the Commvault software, do the following:

1. Add the local storage array in Array Management.

   See Setting Up the Huawei Array Using Array Management.

2. Add the remote storage array in Array Management.

   See Setting Up the Huawei Array Using Array Management.

Note

For File System HyperMetro, follow these steps:

1. Create a new vStore within the FS HyperMetro configuration.

2. Add the service IP (or both management and service IPs) to the vStore created in the previous step.

3. Add the service IP addresses to the Array Host Aliases list under array management on the preferred or primary site.

×

Loading...