# Overriding Old Proxy Computer With a New Proxy Computer During Recall Operations

Archived data (stubs) contain the name of the proxy computer in the reparse data. When you recall a stub, the name of the proxy computer contained in the reparse data is used for the recall operation.

You can switch to a new proxy computer with a better configuration for recall operations.

## Procedure

- To override the old proxy computer name in the reparse data with a new proxy computer, you must add the sRemoteRecallAccessNode additional setting.

Property | Value
--- | ---
Name | sRemoteRecallAccessNode
Category | File system
Type | String
Value | Fully qualified name of the new proxy computer that you want to use for recall operations.

×

Loading...