# Firewall Port Requirements

### CommServe and MediaAgent

The following ports must be opened if the CommServe and MediaAgent are installed in the appliance:

Source Device / Network | Transport Protocol | Port | Purpose
--- | --- | --- | ---
RedHat Enterprise Virtualization | TCP | 80 | For HTTP
RedHat Enterprise Virtualization | TCP | 111 | For NFS export
RedHat Enterprise Virtualization | TCP | 161 | For SNMP
RedHat Enterprise Virtualization | TCP | 389 | For LDAP
RedHat Enterprise Virtualization | TCP | 443 | For HTTPS
RedHat Enterprise Virtualization | TCP | 464 | For Kerberos Authentication
RedHat Enterprise Virtualization | TCP | 636 | For LDAP
RedHat Enterprise Virtualization | TCP | 662 | For RHEV manager
RedHat Enterprise Virtualization | TCP | 875 | For RHEV manager
RedHat Enterprise Virtualization | TCP | 892 | For RHEV manager
RedHat Enterprise Virtualization | TCP | 963 | For RHEV manager
RedHat Enterprise Virtualization | TCP | 965 | For RHEV manager
RedHat Enterprise Virtualization | TCP | 2020 | For RHEV manager
RedHat Enterprise Virtualization | TCP | 2049 | For NFS export
RedHat Enterprise Virtualization | TCP | 2222 | For SSH
RedHat Enterprise Virtualization | TCP | 2223 | For SSH
RedHat Enterprise Virtualization | TCP | 5432 | For PostgreSQL
RedHat Enterprise Virtualization | TCP | 5989 | For CIMOM
RedHat Enterprise Virtualization | TCP | 6081 | For RHEV manager
RedHat Enterprise Virtualization | TCP | 6100 | For RHEV manager
RedHat Enterprise Virtualization | TCP | 5634 - 6166 | For guest console connections
RedHat Enterprise Virtualization | TCP | 5900 - 6923 | For remote guest console access
RedHat Enterprise Virtualization | TCP | 16514 | For libvirt virtual machine migration traffic
RedHat Enterprise Virtualization | TCP | 32769 | For RHEV manager
RedHat Enterprise Virtualization | TCP | 32803 | For RHEV manager
RedHat Enterprise Virtualization | TCP | 24009-24108 | For RHEV functionality
RedHat Enterprise Virtualization | TCP | 49152-49216 | For VDSM virtual machine migration traffic
RedHat Enterprise Virtualization | TCP | 54321 | For RHEV manager
RedHat Enterprise Virtualization | TCP | 54322 | For RHEV manager
RedHat Enterprise Virtualization | UDP | 111 | For NFS export
RedHat Enterprise Virtualization | UDP | 389 | For LDAP
RedHat Enterprise Virtualization | UDP | 464 | For Kerberos Authentication
RedHat Enterprise Virtualization | UDP | 636 | For LDAP
RedHat Enterprise Virtualization | UDP | 2049 | For NFS export
RedHat Enterprise Virtualization | UDP | 5432 | For PostgreSQL
RedHat Enterprise Virtualization | UDP | 5989 | For CIMOM
RedHat Enterprise Virtualization | UDP | 7410 | For RHEV manager
Firewall ports for apache thrift | TCP | 9090 | Apache thrift framework for remote server verification
Firewall ports for avahi | UDP | 37867 | Zero-configuration protocol to discover remote appliance
Firewall ports for avahi | UDP | 37867 | Zero-configuration protocol to discover remote appliance
Firewall ports for avahi | UDP | 5353 | Zero-configurationprotocol to discover remote appliance
Firewall ports for ovirt-console | TCP | 80 | For HTTP
Firewall ports for ovirt-console | TCP | 443 | For HTTPS
Firewall ports for ovirt-console | TCP | 2049 | For NFS
Firewall ports for ovirt-console | TCP | 2222 | For SSH
Firewall ports for ovirt-console | TCP | 6100 | For RHEV manager
Firewall ports for ovirt-console | UDP | 2049 | For NFS
Firewall ports for ovirt-console | UDP | 7410 | For RHEV manager
Firewall ports for glusterfs | TCP | 24007 | For glusterd
Firewall ports for glusterfs | TCP | 24008 | For glusterd RDMA port management
Firewall ports for glusterfs | TCP | 24009 | For glustereventsd
Firewall ports for glusterfs | TCP | 38465 | Gluster NFS service
Firewall ports for glusterfs | TCP | 38466 | Gluster NFS service
Firewall ports for glusterfs | TCP | 38467 | Gluster NFS service
Firewall ports for glusterfs | TCP | 38468 | Gluster NFS service
Firewall ports for glusterfs | TCP | 38469 | Gluster NFS service
Firewall ports for glusterfs | TCP | 49152-49664 | 512 ports for bricks
Commvault services | TCP | 8400 | CVD services
Commvault services | TCP | 8401 | Server Event Manager
Commvault services | TCP | 8402 |
Commvault services | TCP | 8403 | Commvault Firewall
Commvault services | TCP | 8405 |
Commvault services | TCP | 8800 - 8900* | Other services

* 8800-8900 will be reserved using bind-to-open ports option. ** Ports 80,443, and 22 are needed for connections between iRMC and data network. For more information about iRMC ports, refer to Fujitsu manual.

### MediaAgent Only

The following ports must be opened if only the MediaAgent is installed in the appliance:

Source Device / Network | Transport Protocol | Port | Purpose
--- | --- | --- | ---
Firewall ports for apache thrift | TCP | 9090 | Apache thrift framework for remote server verification
Firewall ports for glusterfs | TCP | 24007 | For glusterd
Firewall ports for glusterfs | TCP | 24008 | For glusterd RDMA port management
Firewall ports for glusterfs | TCP | 24009 | For glustereventsd
Firewall ports for glusterfs | TCP | 38465 | Gluster NFS service
Firewall ports for glusterfs | TCP | 38466 | Gluster NFS service
Firewall ports for glusterfs | TCP | 38467 | Gluster NFS service
Firewall ports for glusterfs | TCP | 38468 | Gluster NFS service
Firewall ports for glusterfs | TCP | 38469 | Gluster NFS service
Firewall ports for glusterfs | TCP | 49152-49664 | 512 ports for bricks
Commvault services | TCP | 8400 | CVD services
Commvault services | TCP | 8401 | Server Event Manager
Commvault services | TCP | 8402 |
Commvault services | TCP | 8403 | Commvault Firewall
Commvault services | TCP | 8405 |
Commvault services | TCP | 8800 - 8900* | Other services
Firewall ports for avahi | UDP | 5353 | Zero-configuration protocol to discover remote appliance
Firewall ports for avahi | UDP | 37867 | Zero-configuration protocol to discover remote appliance

* 8800-8900 will be reserved using bind-to-open ports option.

×

Loading...