# Naming Convention for Snapshots Created by the Dell EMC PowerMax/VMAX3/VMAX/Symmetrix Array

The snapshots created by the Dell EMC PowerMax/VMAX3/VMAX/Symmetrix array have the following naming conventions.

Snapshot engine | Configuration | Naming convention | Example
--- | --- | --- | ---
Dell EMC TimeFinder BCV | default | SP_2_JobID_SnapID | SP_2_114038_6641
Dell EMC TimeFinder Clone | default | SP_2_JobID_SnapID | SP_2_5621_109
Dell EMC TimeFinder Snap | default | SP_2_JobID_SnapID | SP_2_5638_110
Dell EMC TimeFinder SnapVX | default | SP_2_JobID_SnapID | SP_2_2255_2059
Dell EMC TimeFinder VP Snap | default | SP_2_JobID_SnapID | SP_2_114031_6629

where:

- SP_2 is a constant value.

- JobID is the Commvault software JobID.

- SnapID is the snapshot ID created by the Commvault software, and corresponds to the primary key of the SMSnap table entry in the CommCell database.

×

Loading...