# Downloading the ISO File for 1-Touch

You can download the ISO file from the Commvault Store. For more information, see 1-Touch ISOs.

## Before You Begin

- You can directly add the drivers to the downloaded ISO file using 1-Touch.exe. For more information, see Adding Drivers to Windows Driver Manager and Adding Windows Drivers for NIC and Mass Storage Devices.

## Procedure

1. Go to the MEDIA KITS on the Commvault Store page.

2. In the 1-Touch section, click the Download button next to the Commvault ISO application.

   CommServe version | Recommended ISO for the restore operation
   --- | ---
   Service Pack 32 and lower | Latest 11.32 ISO
   Service Pack 36 | Latest 11.36 ISO
   Service Pack 11.40 (Minimum CU 16) | Latest 11.40 ISO

   For more information about the supported WinPE versions, see 1-Touch ISOs.

   The software media is downloaded to the location that you specified.

   - If you downloaded the Download Manager, you will see the application executable along with the checksum file.

   - If you downloaded a software disc, you will see the .iso image of the disc.

     Mount the .iso using an appropriate software (for example, MagicISO). Then, use the software media from the mount location.

3. Use the ISO image to boot the client using any one of the following methods:

   - Burn a Live CD.

   - Copy the ISO to a USB drive and connect the USB drive to the client computer that you want to boot. For more information on creating a bootable USB drive, see Create a Bootable USB.

## Related topics

Create a Self-Installing 1-Touch ISO

×

Loading...