# IP Allowlist for Controlling Access to the Command Center

IP allowlist provisions the ability to create a list of IP addresses to permit access to the Command Center. This method allows the Commvault software to deny access to any IP address that is not on the allowlist, ensuring only trusted sources can connect.

You can configure an IP allowlist at the CommCell level and the Company level.

The allowlist supports the following IP adresses:

- A single IPv4 and IPv6 address

- IPv4 and IPv6 address range

- IPv4 and IPv6 CIDR range

×

Loading...