# Configuration of the Inline Replication Feature for the Hitachi Vantara Storage Array

To configure the Hitachi Vantara Inline Replication feature, with the Hitachi Vantara software, you need to set up the replication link between the local array and the remote array. With the Commvault software, you create the backup plan for replication, associate the subclients that you want to protect with the replica copy, and then add and configure the arrays in the Commvault software.

## Configuration Process for Inline Replication

1. To create the Hitachi Universal Replicator (HUR) or the TrueCopy remote replication, use the Command Control Interface (CCI).

   Tip

   Do not use any other interface to create the replication link between the local array and the remote array.

2. Create a backup plan and a snapshot copy on that backup plan.

3. Create the replica copy.

4. Add the local storage array. See Setting Up the Hitachi Vantara Array.

5. Add the remote storage array. See Setting Up the Hitachi Vantara Array.

6. Edit the snapshot configuration properties of the local array.

7. Edit the snapshot configuration properties of the remote array.

×

Loading...