# Add VTL

Use this dialog box to create a virtual tape library (VTL).

VTL Name

Name of the VTL.

Library Vendor

Select the name of the tape library vendor.

Library Type

Select the library that must be emulated.

VDrive Type

Select the drive that must be emulated.

Note

Only a single tape drive type emulation is supported. (Mixed mode libraries are not supported)

Number of VDrives

Select the number of drives that must be emulated.

Drive Start Address

Enter a number as the starting element address to report for the tape drives.

Number of VSlots

Enter the number of storage slots to emulate. The maximum number of storage slots is 60000 per VTL.

Slot Start Address

Enter a number as the starting storage slot.

Number of IE Ports

Enter the number of access ports to emulate. This can be between 0 to 200.

IE Start Address

Enter the number for IE start address.

×

Loading...