# Enabling Retiring of Micropruning Disabled Mountpaths

You can enable retiring of micropruning disabled mountpaths using an additional setting.

## Procedure

- To the CommServe computer, add the bEnableRetireForMicroPruningDisabledMP additional setting as shown in the following table.

  For instructions about adding additional settings from the Command Center, see Adding a CommCell Setting.

  Property | Value
  --- | ---
  Name | bEnableRetireForMicroPruningDisabledMP
  Category | CommServDB.GxGlobalParam
  Type | Boolean
  Value | False

×

Loading...